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VOIP lab experiment#2 Configuring Elastix

Installation and Repair of Telecommunications Equipment









Name of student:	
Group Number:	
Installation and Repair of Telecommunications Equipment
Module 21 Telephone network systems installation

Date:	
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The purpose of the lab is to configure the Elastix software. You will be configuring the following settings:
· Type of installation
· Configure TCP/IP
· Time Zone
· Password
· IPV4 and IPV6
· Hostname configuration
· Time Zone selection



Type of installation 

1- Choose Full install FreePbx 4.211.64 pressing enter
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Configure TCP/IP
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Press tab button to go to OK and then press “enter”
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Just press “enter”
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Time Zone
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Press tab button to go to New york then select Montreal
Press tab button to go to OK and then press “enter”
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[bookmark: _dce27bz6gyo2]Password selecting : use pec12345
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Press tab button to go to Ok and then press “enter”


[image: ]
Press tab button to go to Use Anyway then press “enter”
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Username: root
Password: pec12345






Go to your google chrome and open the ip address showing in the screen.
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Create the admin user: Username: admin
				    Password: admin
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————1 Configure TCP/IP —7M
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Unsupported Harduare Detected F—

This harduare (or a combination
thereof) is not supported by
Cent0S. For more information on
supported harduare, please refer
to http://uww.centos.org/harduare.
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—— Time Zone Selection ———

In which time zome are you located?

America/Montevideo
America/Montreal
America/Montserrat
America/Nassau
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— 1 Root Password —7M

Pick a root password. You must type it
tuice to ensure you know it and do not
make a tuping mistake.
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,—| Root Passuord |—|
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— ] Veak Password b———————

You have provided a weak password: it is based on a dictiomary word
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ent0S release 6.4 (Final)
kernel 2.6.32-358.14.1.e16.i686 on an i686

localhost login: root
Password :

[nterface ethd IP: 192.168.188.119

Please note most tasks should be handled through the FreePBX UI.
fou can access the FreePBX GUI by tuping ome of the above IP’s in to your web br
user .

For support please visit http://uwu. freepbx.org/support-and-professional-service

root@localhost ~1#
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€ > C A Notsecure | 192.168.100.119/admin/config.php

X% rreerixsupport | tsymphony panel || Userpanel |

Welcome to FreePBX Administration!

Inital setup

Please provide the core credentials that will be used to administer your system

Username username
Password password
Confirm Password password
Admin Email address  email address.

Confirm Email address | confirm email

Set up my Account
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Fle Machine View Input Devices Help

Welcome to FreePBX 4.211.64 (Call-Forward)

FreePBX 4.211.64 with Asterisk 11
Full Install
FulT Install
Full Install — Advanced
HA Install — Requires 250G or larger disk

FreePBX 4.211.64 with Asterisk 1.8
Full Install
Full Install — No RAID
Full Install — Advanced
HA Install — Requires 250G or larger disk

No RATD

Press [Tab] to edit options
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