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VOIP lab experiment#4 Configuring Zoiper

Installation and Repair of Telecommunications Equipment









Name of student:	
Group Number:	
Installation and Repair of Telecommunications Equipment
Module 21 Telephone network systems installation

Date:	
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The purpose of the lab is to demonstrate the ability of the students to configure the softphone Zoiper by assigning an extension created in lab#3.
1- To start assigning an extension, you need to open the software.
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2- Click on continue as a free user

3- You want to assign an extension to the softphone. ONLY 1 Extension can be assigned to 1 softphone at a time.
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4- In the first rectangle assign one of the 3 extensions you have created in lab#3. (1000, 2000 or 3000). In the 2nd rectangle enter the password of the extension: pec123
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5- The 2nd rectangle password is pec123, click on login
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6- In the rectangle, enter your PBX IP address, then click on Next
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7- Press skip
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8- The SIP UDP should be in green colour, found. Click next
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9- The green arrow means your extension has properly been assigned to the softphone.
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Username and password

If you already have a VoIP account, please enter your login
credentials to the left.

Most often these are provided either by your VolIP provider, or
by your system administrator for your office’s IP PBX.

*we will try to automaticalyfind the necessary configuration for your account. If such does
ot exist i our database, you'l be asked to enter specific detalk.
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Username and password

Ifyou already have a VoIP account, please enter your login
credentials to the left.

Most often these are provided either by your VoIP provider, or
by your system administrator for your office’s IP PBX.

Create account “we will try to automatically ind the necessary configuration for your account. I such does.

ot exist i our database, you'l be asked to enter specific detals.
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Fill in your hostname

and select your

provider from the list

Hostname

This could also be called ‘Domain’, SIP server’, ‘Registrar’ or
‘SIP Proxy’. For example 'sip.example.com’ or
123.21.123.32:5060°.

You can also just search for the name of your provider, maybe
we know the settings. If not - you'll be able to set it up
manually.
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Authentication and
Outbound pro:

Authentication username

Not sure if you need this? Ask your VoIP provider or system
administrator about the requirements for your office PBX.

Outbound proxy

This is typically not required. However, in some special
environments it is needed for network access.
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Success!

We have found some transport type(s) that are available for
your configuration.

The default ones marked with ‘Recommended: are priority
ordered based on the stability and security of said protocols.
However, you are free to choose manually one of the options
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LESTER B. PEARSON
Pearson Electrotechnology Centre
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.@ ZoiPer

You are running Zoiper Community Edition
Free for non commercial use

Activate your PRO license.

OR

Continue as a Free user





