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VOIP lab experiment#6
Creating a trunk in PBX
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The purpose of the lab is to create a trunk in the PBX. A trunk is the phone number of the supplier such as Bell, Videotron, etc…
Go to the trunk, inside of the menu connectivity, and then click on add a sip trunk
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1- [bookmark: _heading=h.gjdgxs]Enter the following information:[image: ]
OUTGOING********
host=172.16.0.2
username=51455500xx
fromuser=51455500xx
secret=pec123
type=peer
context=from-trunk
insecure=very
**************


Incoming settings******************
      USER CONTEXT 51455500xx
type=peer
secret=pec123
host=172.16.0.2
allow=all
insecure=very
*************************************









Register String:
51455500xx:pec123@172.16.0.2/51455500xx

click on submit and then apply configuration.
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