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The purpose of the lab is to demonstrate the ability of the students to configure the virtual box.

Oracle VM VirtualBox is cross-platform virtualization software. It allows users to extend their existing computer to run multiple operating systems including Microsoft Windows, Mac OS X, Linux, and Oracle Solaris, at the same time.


1- Open Virtual box software on your desktop[image: ]
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2- Click on “machine”, and choose “new”[image: ]

















A window like this will appear.[image: ]


3- Setup the following:

a. Name: Elastix
b. Type: Linux
c. Version: RED Hat 32-bit
d. Press Next
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4- For memory size, choose 1024MB. Click next[image: ]





















5- Choose create a virtual hard disk now and then click create[image: ]


















6- Choose VDI (virtual box disk image), and then click next
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7- CHoose “dynamically allocated”. Then click next[image: ][image: ]





















8- You want to create a hard disk of 8GB, so click on create.
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Once all the previous steps are completed, you can now access to the main page of the virtual box and configure. You will be configuring 2 different settings:
· Network
· Storage[image: ]




























Click on settings to choose the configuration that you want to modify.
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Network Settings
In this setting, you will be prompt to set the attached to and the name of the adapter:
[image: ]Attached to: Bridge Adapter
Name: Wireless Adapter




Click on ok once this setup is completed.
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Storage setup
In controller: IDE, click on empty[image: ]
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Browse and attached your FreePBX iso file[image: ]



























Click on ok to go back in the main window and start the virtual Box simulation
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A screen like this should appear once you start the virtual box machine.

[image: ]
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€ Create Virtual Machine

Memory size
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Hard disk

1F you wish you can add a virtual hard disk to the new machine. You can ether
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Hard disk file type
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€ Create Virtual Hard Disk
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3 Oracle VM VirtualBox Manager
Fie Machine Help
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