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VOIP lab experiment#10
Uploading the wav message into the system recordings
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The purpose of the lab is to upload the wav message from laboratory 7 into the system recording.

1- Go to system recordings located into admin menu:
[image: ]
1- Click on browse and choose the audio file that you saved earlier and the click on upload

2- Click on save

3- Submit changes and then click on apply config.
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Step 1: Record or upload

If you wish to make and verify recordings from your phone, please enter your extension number here: [0

Alternatively, upload a recording in any supported asterisk format. Note that if you're using wav, (eg, recorded with Microsoft Recorder) the file must be PCM Encoded, 16 Bits, at 8000Hz:
[Choose File | No file chosen | upload |

Step 2: Name

Name this Recording

Click "SAVE" when you ar satisfied with your recording | Save
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