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Module 21 
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VOIP lab experiment#5
Installing IP Phone


Installation and Repair of Telecommunications Equipment






Name of student:________________
Group Number:_________________
Date:_________________________





The purpose of the lab is to install an IP Phone in the PBX. 
Install a patch cable to make the IP Phone work.
Check the phone IP address  using the menu key then status (1)
Open Google Chrome and type the IP address.

1- The default User is admin and the password is admin 
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2- Complete all information based on extension that you created
3- Click Confirm
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